    001/*
    002 * Licensed to the Apache Software Foundation (ASF) under one or more
    003 * contributor license agreements.  See the NOTICE file distributed with
    004 * this work for additional information regarding copyright ownership.
    005 * The ASF licenses this file to You under the Apache License, Version 2.0
    006 * (the "License"); you may not use this file except in compliance with
    007 * the License.  You may obtain a copy of the License at
    008 *
    009 *      http://www.apache.org/licenses/LICENSE-2.0
    010 *
    011 * Unless required by applicable law or agreed to in writing, software
    012 * distributed under the License is distributed on an "AS IS" BASIS,
    013 * WITHOUT WARRANTIES OR CONDITIONS OF ANY KIND, either express or implied.
    014 * See the License for the specific language governing permissions and
    015 * limitations under the License.
    016 */
    017package org.apache.commons.imaging.formats.tiff.photometricinterpreters;
    018
    019import java.io.IOException;
    020
    021import org.apache.commons.imaging.ImageReadException;
    022import org.apache.commons.imaging.common.ImageBuilder;
    023
    024public class PhotometricInterpreterRgb extends PhotometricInterpreter {
    025    public PhotometricInterpreterRgb(final int samplesPerPixel,
    026            final int[] bitsPerSample, final int predictor, final int width, final int height) {
    027        super(samplesPerPixel, bitsPerSample, predictor, width, height);
    028    }
    029
    030    @Override
    031    public void interpretPixel(final ImageBuilder imageBuilder, final int[] samples, final int x,
    032            final int y) throws ImageReadException, IOException {
    033        final int red = samples[0];
    034        final int green = samples[1];
    035        final int blue = samples[2];
    036
    037        final int alpha = 0xff;
    038        final int rgb = (alpha << 24) | (red << 16) | (green << 8) | (blue << 0);
    039        imageBuilder.setRGB(x, y, rgb);
    040
    041    }
    042}