    001/*
    002 * Licensed to the Apache Software Foundation (ASF) under one or more
    003 * contributor license agreements.  See the NOTICE file distributed with
    004 * this work for additional information regarding copyright ownership.
    005 * The ASF licenses this file to You under the Apache License, Version 2.0
    006 * (the "License"); you may not use this file except in compliance with
    007 * the License.  You may obtain a copy of the License at
    008 *
    009 *     https://www.apache.org/licenses/LICENSE-2.0
    010 *
    011 * Unless required by applicable law or agreed to in writing, software
    012 * distributed under the License is distributed on an "AS IS" BASIS,
    013 * WITHOUT WARRANTIES OR CONDITIONS OF ANY KIND, either express or implied.
    014 * See the License for the specific language governing permissions and
    015 * limitations under the License.
    016 */
    017package org.apache.commons.configuration2.sync;
    018
    019/**
    020 * <p>
    021 * An interface controlling synchronization of configuration instances.
    022 * </p>
    023 * <p>
    024 * Each {@code Configuration} object derived from {@link org.apache.commons.configuration2.AbstractConfiguration
    025 * AbstractConfiguration} has an associated {@code Synchronizer} object. Before an operation on the configuration is
    026 * performed (for example a property read or an update), the {@code Synchronizer} is invoked. Depending on the concrete
    027 * implementation of the {@code Synchronizer} used, the configuration can be made thread-safe.
    028 * </p>
    029 * <p>
    030 * Whether a configuration has to be thread-safe or not is a matter of a concrete use case. For instance, an application
    031 * that just reads some configuration settings on startup does need a thread-safe configuration implementation. A
    032 * configuration in contrast which is shared between multiple components and updated concurrently should better be
    033 * thread-safe. In order to satisfy both kinds of use cases, the support for thread-safety has been extracted out of the
    034 * configuration implementation and refactored into this {@code Synchronizer} interface. By assigning different
    035 * {@code Synchronizer} implementations to a configuration instance, the instance's support for concurrent access can be
    036 * adapted to the concrete use case.
    037 * </p>
    038 * <p>
    039 * The methods defined by this interface are similar to a <em>read-write lock</em>. The {@code Synchronizer} is notified
    040 * when read or write operations start and end. A concrete implementation can then apply a specific policy to decide
    041 * when threads need to block or when access to the configuration for the desired operation is granted.
    042 * </p>
    043 *
    044 * @since 2.0
    045 */
    046public interface Synchronizer {
    047
    048    /**
    049     * Notifies this {@code Synchronizer} that the current thread is going to start a read operation on the managed
    050     * configuration. This call can block if a concrete implementation decides that the thread has to wait until a specific
    051     * condition is fulfilled.
    052     */
    053    void beginRead();
    054
    055    /**
    056     * Notifies this {@code Synchronizer} that the current thread is going to start a write operation on the managed
    057     * configuration. This call may block. For instance, a concrete implementation may suspend the thread until all read
    058     * operations currently active are finished,
    059     */
    060    void beginWrite();
    061
    062    /**
    063     * Notifies this {@code Synchronizer} that the current thread has finished its read operation. This may cause other
    064     * waiting threads to be granted access to the managed configuration.
    065     */
    066    void endRead();
    067
    068    /**
    069     * Notifies this {@code Synchronizer} that the current thread has finished its write operation. This may cause other
    070     * waiting threads to be granted access to the managed configuration.
    071     */
    072    void endWrite();
    073}