    001package org.apache.commons.net.ntp;
    002/*
    003 * Licensed to the Apache Software Foundation (ASF) under one or more
    004 * contributor license agreements.  See the NOTICE file distributed with
    005 * this work for additional information regarding copyright ownership.
    006 * The ASF licenses this file to You under the Apache License, Version 2.0
    007 * (the "License"); you may not use this file except in compliance with
    008 * the License.  You may obtain a copy of the License at
    009 *
    010 *      http://www.apache.org/licenses/LICENSE-2.0
    011 *
    012 * Unless required by applicable law or agreed to in writing, software
    013 * distributed under the License is distributed on an "AS IS" BASIS,
    014 * WITHOUT WARRANTIES OR CONDITIONS OF ANY KIND, either express or implied.
    015 * See the License for the specific language governing permissions and
    016 * limitations under the License.
    017 */
    018
    019
    020/***
    021 * Common NtpUtils Helper class.
    022 *
    023 */
    024public final class NtpUtils {
    025
    026    /***
    027      * Returns 32-bit integer address to IPv4 address string "%d.%d.%d.%d" format.
    028      *
    029      * @param address  the 32-bit address
    030      * @return  the raw IP address in a string format.
    031      */
    032     public static String getHostAddress(int address)
    033     {
    034          return ((address >>> 24) & 0xFF) + "." +
    035                 ((address >>> 16) & 0xFF) + "." +
    036                 ((address >>>  8) & 0xFF) + "." +
    037                 ((address >>>  0) & 0xFF);
    038     }
    039
    040    /***
    041     * Returns NTP packet reference identifier as IP address.
    042     *
    043     * @param packet  NTP packet
    044     * @return  the packet reference id (as IP address) in "%d.%d.%d.%d" format.
    045     */
    046     public static String getRefAddress(NtpV3Packet packet)
    047     {
    048         int address = (packet == null) ? 0 : packet.getReferenceId();
    049         return getHostAddress(address);
    050     }
    051
    052    /***
    053     * Get refId as reference clock string (e.g. GPS, WWV, LCL). If string is
    054     * invalid (non-ASCII character) then returns empty string "".
    055     * For details refer to the <A HREF="http://www.eecis.udel.edu/~mills/ntp/html/refclock.html#list">Comprehensive
    056     * List of Clock Drivers</A>.
    057     *
    058     * @param message the message to check
    059     * @return reference clock string if primary NTP server
    060     */
    061    public static String getReferenceClock(NtpV3Packet message) {
    062        if (message == null) {
    063            return "";
    064        }
    065        int refId = message.getReferenceId();
    066        if (refId == 0) {
    067            return "";
    068        }
    069        StringBuilder buf = new StringBuilder(4);
    070        // start at highest-order byte (0x4c434c00 -> LCL)
    071        for (int shiftBits = 24; shiftBits >= 0; shiftBits -= 8)
    072        {
    073            char c = (char) ((refId >>> shiftBits) & 0xff);
    074            if (c == 0) { // 0-terminated ASCII string
    075                break;
    076            }
    077            if (!Character.isLetterOrDigit(c)) {
    078                return "";
    079            }
    080            buf.append(c);
    081        }
    082        return buf.toString();
    083    }
    084
    085    /***
    086     * Return human-readable name of message mode type (RFC 1305).
    087     *
    088     * @param mode the mode type
    089     * @return mode name
    090     */
    091    public static String getModeName(int mode)
    092    {
    093        switch (mode) {
    094            case NtpV3Packet.MODE_RESERVED:
    095                return "Reserved";
    096            case NtpV3Packet.MODE_SYMMETRIC_ACTIVE:
    097                return "Symmetric Active";
    098            case NtpV3Packet.MODE_SYMMETRIC_PASSIVE:
    099                return "Symmetric Passive";
    100            case NtpV3Packet.MODE_CLIENT:
    101                return "Client";
    102            case NtpV3Packet.MODE_SERVER:
    103                return "Server";
    104            case NtpV3Packet.MODE_BROADCAST:
    105                return "Broadcast";
    106            case NtpV3Packet.MODE_CONTROL_MESSAGE:
    107                return "Control";
    108            case NtpV3Packet.MODE_PRIVATE:
    109                return "Private";
    110            default:
    111                return "Unknown";
    112        }
    113    }
    114
    115}