//
//  Licensed to the Apache Software Foundation (ASF) under one or more
//  contributor license agreements.  See the NOTICE file distributed with
//  this work for additional information regarding copyright ownership.
//  The ASF licenses this file to You under the Apache License, Version 2.0
//  (the "License"); you may not use this file except in compliance with
//  the License.  You may obtain a copy of the License at
//
//      https://www.apache.org/licenses/LICENSE-2.0
//
//  Unless required by applicable law or agreed to in writing, software
//  distributed under the License is distributed on an "AS IS" BASIS,
//  WITHOUT WARRANTIES OR CONDITIONS OF ANY KIND, either express or implied.
//  See the License for the specific language governing permissions and
//  limitations under the License.
//

// Code generated by code-generation. DO NOT EDIT.

[cols="2,2a,2a,2a,4a"]
|===
|Name |Type |Default Value |Required |Description
|Name 4+|Beckhoff TwinCat ADS
|Code 4+|`ads`
|Maven Dependency 4+|

[subs=attributes+]
----
<dependency>
  <groupId>org.apache.plc4x</groupId>
  <artifactId>plc4j-driver-ads</artifactId>
  <version>{page-component-version}</version>
</dependency>
----
|Default Transport 4+|`tcp`
|Supported Transports 4+|
 - `tcp`
5+|Config options:
|`target-ams-net-id` |STRING | |required |AMS-Net-Id of the target. An AMS-Net-Id has the regular format of an IPv4 IP-Address, however with 6 segments instead of 4.
|`target-ams-port` |INT | |required |AMS port of the target.
|`source-ams-net-id` |STRING | |required |AMS-Net-Id of the source. An AMS-Net-Id has the regular format of an IPv4 IP-Address, however with 6 segments instead of 4.
|`source-ams-port` |INT | |required |AMS port of the source.
|`timeout-request` |INT |4000| |Default timeout for all types of requests.
|`load-symbol-and-data-type-tables` |BOOLEAN |true| |Configures, if when connecting the data-type- and symbol-table should be read. This is an optimization that can help in cases, where the PLC program is pretty large and downloading the full tables is causing problems. When disabled, symbolic addresses will manually be resolved as soon as an address is used.
5+|Transport config options:
5+|
+++
<h4>tcp</h4>
+++
|`tcp.keep-alive` |BOOLEAN |false| |Should keep-alive packets be sent?
|`tcp.no-delay` |BOOLEAN |true| |Should packets be sent instantly or should we give the OS some time to aggregate data.
|`tcp.default-timeout` |INT |1000| |Timeout after which a connection will be treated as disconnected.
|===
