//
//  Licensed to the Apache Software Foundation (ASF) under one or more
//  contributor license agreements.  See the NOTICE file distributed with
//  this work for additional information regarding copyright ownership.
//  The ASF licenses this file to You under the Apache License, Version 2.0
//  (the "License"); you may not use this file except in compliance with
//  the License.  You may obtain a copy of the License at
//
//      http://www.apache.org/licenses/LICENSE-2.0
//
//  Unless required by applicable law or agreed to in writing, software
//  distributed under the License is distributed on an "AS IS" BASIS,
//  WITHOUT WARRANTIES OR CONDITIONS OF ANY KIND, either express or implied.
//  See the License for the specific language governing permissions and
//  limitations under the License.
//

== Capture Replay Tool

Some times it is difficult to track down problems where they occur.

Especially when it comes to passive mode drivers, problems sometimes are difficult to track down.

However with this tool it's easy to to this work by simply recording a WireShark recording of the network traffic and then replaying this from another device.

In my setup I use an ordinary Raspberry PI to replay a previously recorded capture and then to work on the passive mode drivers as if you were connected to the real thing.

=== Usage

In order to replay a previously recorded network capture, you need:

- The `PCAPNG` capture itself
- The name of the network device (like shown by `ifconfig` or `ipconfig` (on Windows))
- An optional replay speed (if omitted a value of `1` is assumed which is real-time)

Run the application like this:

    java -jar plc4j-capture-replay-0.7.0-SNAPSHOT.jar