# Package org.apache.activemq.artemis.jms.bridge

- Interface Summary
  Interface | Description
  --- | ---
  ActiveMQJMSBridgeLogger | Logger Code 34 each message id must be 6 digits long starting with 34, the 3rd digit donates the level so INF0 1 WARN 2 DEBUG 3 ERROR 4 TRACE 5 FATAL 6 so an INFO message would be 341000 to 341999
  ConnectionFactoryFactory |
  DestinationFactory |
  JMSBridge |
  JMSBridgeControl |

- Enum Summary
  Enum | Description
  --- | ---
  QualityOfServiceMode | Quality of server (QoS) levels

Copyright © 2020 The Apache Software Foundation. All rights reserved.