org.apache.sis.storage.gps

## Enum Fix

- Object
- - Enum<Fix>
  - - Fix

- All Implemented Interfaces:
    Serializable, Comparable<Fix>

      public enum Fix
      extends Enum<Fix>

  Type of GPS fix (position derived from measuring external reference points). The Standard Positioning Service (SPS) can be two- or three-dimensional, or use differential GPS for increased accuracy. The Precise Positioning Service (PPS) is a military signal.

  This enumeration value can be encoded in GPS Exchange Format (GPX) with the following strings: `"none"`, `"2d"`, `"3d"`, `"dgps"` and `"pps"`. When reading such data, `Fix` instances can be a property value of the features returned by the GPX reader.

  Since:
    0.8

  Defined in the `sis-xmlstore` module

- - ### Enum Constant Summary

    Enum Constants
    Enum Constant and Description
    `DIFFERENTIAL` Differential Global Positioning Service (DGPS) used.
    `NONE` GPS has no fix.
    `PRECISE` Precise Positioning Service (PPS) used.
    `THREE_DIMENSIONAL` Three-dimensional fix.
    `TWO_DIMENSIONAL` Two-dimensional fix.

  - ### Method Summary

    All Methods Static Methods Instance Methods Concrete Methods
    Modifier and Type | Method and Description
    --- | ---
    `static Fix` | `fromGPX(String name)` Returns the enumeration value from the given GPX name, or `null` if none.
    `String` | `toGPX()` Returns the string representation in GPS Exchange Format (GPX).
    `static Fix` | `valueOf(String name)` Returns the enum constant of this type with the specified name.
    `static Fix[]` | `values()` Returns an array containing the constants of this enum type, in the order they are declared.

    - ### Methods inherited from class Enum

      `clone, compareTo, equals, finalize, getDeclaringClass, hashCode, name, ordinal, toString, valueOf`

    - ### Methods inherited from class Object

      `getClass, notify, notifyAll, wait, wait, wait`

- - ### Enum Constant Detail

    - #### NONE

          public static final Fix NONE

      GPS has no fix. Note that this is a different meaning than "the fix information is unknown".

    - #### TWO_DIMENSIONAL

          public static final Fix TWO_DIMENSIONAL

      Two-dimensional fix. This requires the signal of at least 3 satellites.

    - #### THREE_DIMENSIONAL

          public static final Fix THREE_DIMENSIONAL

      Three-dimensional fix. This requires the signal of at least 4 satellites.

    - #### DIFFERENTIAL

          public static final Fix DIFFERENTIAL

      Differential Global Positioning Service (DGPS) used.
      See Also:
        Differential GPS on Wikipedia

    - #### PRECISE

          public static final Fix PRECISE

      Precise Positioning Service (PPS) used. This is a military signal. (Note: the alternative is Standard Positioning Service – SPS).

  - ### Method Detail

    - #### values

          public static Fix[] values()

      Returns an array containing the constants of this enum type, in the order they are declared. This method may be used to iterate over the constants as follows:

          for (Fix c : Fix.values())
              System.out.println(c);

      Returns:
        an array containing the constants of this enum type, in the order they are declared

    - #### valueOf

          public static Fix valueOf(String name)

      Returns the enum constant of this type with the specified name. The string must match exactly an identifier used to declare an enum constant in this type. (Extraneous whitespace characters are not permitted.)
      Parameters:
        `name` - the name of the enum constant to be returned.
      Returns:
        the enum constant with the specified name
      Throws:
        `IllegalArgumentException` - if this enum type has no constant with the specified name
        `NullPointerException` - if the argument is null

    - #### fromGPX

          public static Fix fromGPX(String name)

      Returns the enumeration value from the given GPX name, or `null` if none. Recognized values are `"none"`, `"2d"`, `"3d"`, `"dgps"` and `"pps"`, ignoring case.
      Parameters:
        `name` - the GPX name (case insensitive) for which to get an enumeration value.
      Returns:
        the enumeration value for the given GPX name, or `null` if the given name was `null` or unrecognized.

    - #### toGPX

          public String toGPX()

      Returns the string representation in GPS Exchange Format (GPX). Returned value can be `"none"`, `"2d"`, `"3d"`, `"dgps"` or `"pps"`,
      Returns:
        the GPX enumeration value.

Copyright © 2010–2017 The Apache Software Foundation. All rights reserved.